{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":225,"n_cols":19,"rows_kept":225,"merged":[[0,1,0,18]],"flags":["formulas_cached_only"]}
[null,"附件1\n2021年阳江市重点监控企业污染源（废水重点）监督性监测结果\n"]
["序号","企业名称","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
[1,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","氨氮（NH3-N）","2021-11-02",0,null,null,10.9,null,null,"mg/L","否",null,null,"否"]
[2,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","化学需氧量","2021-11-02",0,null,null,18,250,null,"mg/L","否",null,null,"是"]
[3,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总镉","2021-11-02",0,null,null,0.00018,0.1,null,"mg/L","否",null,null,"是"]
[4,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总余氯","2021-11-02",0,null,null,2.06,null,null,"mg/L","否",null,null,"否"]
[5,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","动植物油","2021-11-02",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[6,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","悬浮物","2021-11-02",0,null,null,8,60,null,"mg/L","否",null,null,"是"]
[7,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","挥发酚","2021-11-02",0,null,null,"<0.010",1,null,"mg/L","否",null,null,"是"]
[8,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","色度","2021-11-02",0,null,null,2,null,null,"倍","否",null,null,"否"]
[9,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","pH值","2021-11-02",0,null,null,6.8,9,6,"无量纲","否",null,null,"是"]
[10,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","阴离子表面活性剂（LAS）","2021-11-02",0,null,null,"<0.05",10,null,"mg/L","否",null,null,"是"]
[11,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总铅","2021-11-02",0,null,null,"<0.00009",1,null,"mg/L","否",null,null,"是"]
[12,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","粪大肠菌群","2021-11-02",0,null,null,0,5000,null,"个/L","否",null,null,"是"]
[13,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","氰化物（总氰化合物）","2021-11-02",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[14,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","石油类","2021-11-02",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[15,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总砷","2021-11-02",0,null,null,0.00069,0.5,null,"mg/L","否",null,null,"是"]
[16,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总铬","2021-11-02",0,null,null,"<0.004",1.5,null,"mg/L","否",null,null,"是"]
[17,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总银","2021-11-02",0,null,null,"<0.00004",0.5,null,"mg/L","否",null,null,"是"]
[18,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","六价铬","2021-11-02",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[19,"阳西县人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","五日生化需氧量","2021-11-02",0,null,null,6,100,null,"mg/L","否",null,null,"是"]
[20,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆企业","废水监测点1(DW001)","五日生化需氧量","2021-03-10",0,null,319,5.8,40,null,"mg/L","否",null,null,"是"]
[21,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆企业","废水监测点1(DW001)","氨氮（NH3-N）","2021-03-10",0,null,6.89,0.657,16,null,"mg/L","否",null,null,"是"]
[22,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","废水监测点1(DW001)","pH值","2021-03-10",0,null,6.8,6.9,9,6,"无量纲","否",null,null,"是"]
[23,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,造纸企业","废水监测点1(DW001)","总磷（以P计）","2021-03-10",0,null,0.17,0.03,1.6,null,"mg/L","否",null,null,"是"]
[24,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","废水监测点1(DW001)","悬浮物","2021-03-10",0,null,588,8,60,null,"mg/L","否",null,null,"是"]
[25,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,造纸企业","废水监测点1(DW001)","总氮（以N计）","2021-03-10",0,null,12.9,2.36,24,null,"mg/L","否",null,null,"是"]
[26,"维达护理用品（广东）有限公司","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","废水监测点1(DW001)","化学需氧量","2021-03-10",0,null,1160,21,160,null,"mg/L","否",null,null,"是"]
[27,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","总排放口(DW001)","总磷（以P计）","2021-01-06",0,null,1.24,0.08,0.5,null,"mg/L","否",null,null,"是"]
[28,"阳西捷晖净水有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","总排放口(DW001)","化学需氧量","2021-01-06",0,null,126,26,40,null,"mg/L","否",null,null,"是"]
[29,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","总氮（以N计）","2021-01-06",0,null,23.1,8.75,15,null,"mg/L","否",null,null,"是"]
[30,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","悬浮物","2021-01-06",0,null,83,4,10,null,"mg/L","否",null,null,"是"]
[31,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","氨氮（NH3-N）","2021-01-06",0,20,17.2,0.429,"5;8",null,"mg/L","否",null,null,"是"]
[32,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","总排放口(1)","氨氮（NH3-N）","2021-04-06",0,25,35.1,0.589,5,null,"mg/L","否",null,null,"是"]
[33,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","悬浮物","2021-04-06",0,null,104,7,10,null,"mg/L","否",null,null,"是"]
[34,"阳西捷晖净水有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","总排放口(1)","化学需氧量","2021-04-06",0,null,213,5,40,null,"mg/L","否",null,null,"是"]
[35,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","总氮（以N计）","2021-04-06",0,null,40.5,4.54,15,null,"mg/L","否",null,null,"是"]
[36,"阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","总排放口(1)","总磷（以P计）","2021-04-06",0,null,5.12,0.11,0.5,null,"mg/L","否",null,null,"是"]
[37,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","五日生化需氧量","2021-12-07",0,null,null,14,100,null,"mg/L","否",null,null,"是"]
[38,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","挥发酚","2021-12-07",0,null,null,"<0.01",1,null,"mg/L","否",null,null,"是"]
[39,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","动植物油","2021-12-07",0,null,null,0.4,20,null,"mg/L","否",null,null,"是"]
[40,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总镉","2021-12-07",0,null,null,"<0.00005",0.1,null,"mg/L","否",null,null,"是"]
[41,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总银","2021-12-07",0,null,null,"<0.00004",0.5,null,"mg/L","否",null,null,"是"]
[42,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","石油类","2021-12-07",0,null,null,0.08,20,null,"mg/L","否",null,null,"是"]
[43,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","粪大肠菌群","2021-12-07",0,null,null,3500,5000,null,"个/L","否",null,null,"是"]
[44,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","六价铬","2021-12-07",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[45,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","化学需氧量","2021-12-07",0,null,null,45,250,null,"mg/L","否",null,null,"是"]
[46,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总砷","2021-12-07",0,null,null,0.00083,0.5,null,"mg/L","否",null,null,"是"]
[47,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","悬浮物","2021-12-07",0,null,null,9,60,null,"mg/L","否",null,null,"是"]
[48,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","氰化物（总氰化合物）","2021-12-07",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[49,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","阴离子表面活性剂（LAS）","2021-12-07",0,null,null,"<0.05",10,null,"mg/L","否",null,null,"是"]
[50,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总铅","2021-12-07",0,null,null,0.00138,1,null,"mg/L","否",null,null,"是"]
[51,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","pH值","2021-12-07",0,null,null,6.9,9,6,"无量纲","否",null,null,"是"]
[52,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总汞","2021-12-07",0,null,null,0.0004,0.05,null,"mg/L","否",null,null,"是"]
[53,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","总铬","2021-12-07",0,null,null,"<0.004",1.5,null,"mg/L","否",null,null,"是"]
[54,"阳西总医院妇女儿童医院（阳西县妇幼保健院）","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(1)","氨氮（NH3-N）","2021-11-02",0,null,null,46.2,15,null,"mg/L","否",null,null,"否"]
[55,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","氨氮（NH3-N）","2021-11-03",0,null,null,14.5,null,null,"mg/L","否",null,null,"否"]
[56,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总铅","2021-11-03",0,null,null,"<0.00009",1,null,"mg/L","否",null,null,"是"]
[57,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","动植物油","2021-11-03",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[58,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","六价铬","2021-11-03",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[59,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","悬浮物","2021-11-03",0,null,null,9,60,null,"mg/L","否",null,null,"是"]
[60,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","石油类","2021-11-03",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[61,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","氰化物（总氰化合物）","2021-11-03",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[62,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","pH值","2021-11-03",0,null,null,7.4,9,6,"无量纲","否",null,null,"是"]
[63,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总砷","2021-11-03",0,null,null,0.00164,0.5,null,"mg/L","否",null,null,"是"]
[64,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","粪大肠菌群","2021-11-03",0,null,null,1700,5000,null,"个/L","否",null,null,"是"]
[65,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总镉","2021-11-03",0,null,null,0.00012,0.1,null,"mg/L","否",null,null,"是"]
[66,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总银","2021-11-03",0,null,null,"<0.00004",0.5,null,"mg/L","否",null,null,"是"]
[67,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总铬","2021-11-03",0,null,null,"<0.004",1.5,null,"mg/L","否",null,null,"是"]
[68,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","阴离子表面活性剂（LAS）","2021-11-03",0,null,null,"<0.05",10,null,"mg/L","否",null,null,"是"]
[69,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","五日生化需氧量","2021-11-03",0,null,null,2.8,100,null,"mg/L","否",null,null,"是"]
[70,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总汞","2021-11-03",0,null,null,0.00028,0.05,null,"mg/L","否",null,null,"是"]
[71,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","总余氯","2021-11-03",0,null,null,0.012,null,null,"mg/L","否",null,null,"否"]
[72,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","色度","2021-11-03",0,null,null,2,null,null,"倍","否",null,null,"否"]
[73,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","挥发酚","2021-11-03",0,null,null,"<0.010",1,null,"mg/L","否",null,null,"是"]
[74,"阳西总医院第二人民医院（阳西县儒洞镇中心卫生院）","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放监测口(DW001)","化学需氧量","2021-11-03",0,null,null,8,250,null,"mg/L","否",null,null,"是"]
[75,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","总氮（以N计）","2021-01-06",0,null,37.5,5.64,20,null,"mg/L","否",null,null,"是"]
[76,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","氨氮（NH3-N）","2021-01-06",0,20,31.5,2.38,"8;15",null,"mg/L","否",null,null,"是"]
[77,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","排放口","总磷（以P计）","2021-01-06",0,null,6.27,0.73,1,null,"mg/L","否",null,null,"是"]
[78,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","悬浮物","2021-01-06",0,null,65,8,20,null,"mg/L","否",null,null,"是"]
[79,"阳西中炬水务有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","排放口","化学需氧量","2021-01-06",0,null,209,35,40,null,"mg/L","否",null,null,"是"]
[80,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","氨氮（NH3-N）","2021-04-06",0,25,52.8,0.463,"8;15",null,"mg/L","否",null,null,"是"]
[81,"阳西中炬水务有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","排放口(DW001)","化学需氧量","2021-04-06",0,null,235,8,40,null,"mg/L","否",null,null,"是"]
[82,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","悬浮物","2021-04-06",0,null,63,6,20,null,"mg/L","否",null,null,"是"]
[83,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","排放口(DW001)","总磷（以P计）","2021-04-06",0,null,5.26,0.7,1,null,"mg/L","否",null,null,"是"]
[84,"阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","总氮（以N计）","2021-04-06",0,null,57.1,8.68,20,null,"mg/L","否",null,null,"是"]
[85,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","化学需氧量","2021-09-28",0,null,null,86,90,null,"mg/L","否",null,null,"是"]
[86,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","石油类","2021-09-28",0,null,null,"<0.06",5,null,"mg/L","否",null,null,"是"]
[87,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水总排放口(DW001)","动植物油","2021-09-28",0,null,null,0.44,10,null,"mg/L","否",null,null,"是"]
[88,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","悬浮物","2021-09-28",0,null,null,12,60,null,"mg/L","否",null,null,"是"]
[89,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","五日生化需氧量","2021-09-28",0,null,null,27.8,20,null,"mg/L","是",0.39,null,"是"]
[90,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","氨氮（NH3-N）","2021-09-28",0,null,null,0.862,10,null,"mg/L","否",null,null,"是"]
[91,"阳江珠江啤酒分装有限公司","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水总排放口(DW001)","pH值","2021-09-28",0,null,null,7.09,9,6,"mg/L","否",null,null,"是"]
[92,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","化学需氧量","2021-11-02",0,null,null,8,250,null,"mg/L","否",null,null,"是"]
[93,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总铬","2021-11-02",0,null,null,"<0.004",1.5,null,"mg/L","否",null,null,"是"]
[94,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","五日生化需氧量","2021-11-02",0,null,null,4.4,100,null,"mg/L","否",null,null,"是"]
[95,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总铅","2021-11-02",0,null,null,"<0.00009",1,null,"mg/L","否",null,null,"是"]
[96,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","粪大肠菌群","2021-11-02",0,null,null,130,5000,null,"个/L","否",null,null,"是"]
[97,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","阴离子表面活性剂（LAS）","2021-11-02",0,null,null,"<0.05",10,null,"mg/L","否",null,null,"是"]
[98,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","pH值","2021-11-02",0,null,null,7.7,9,6,"无量纲","否",null,null,"是"]
[99,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总砷","2021-11-02",0,null,null,0.00288,0.5,null,"mg/L","否",null,null,"是"]
[100,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","动植物油","2021-11-02",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[101,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总镉","2021-11-02",0,null,null,0.00063,0.1,null,"mg/L","否",null,null,"是"]
[102,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总汞","2021-11-02",0,null,null,0.00018,0.05,null,"mg/L","否",null,null,"是"]
[103,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","悬浮物","2021-11-02",0,null,null,13,60,null,"mg/L","否",null,null,"是"]
[104,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","石油类","2021-11-02",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[105,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","六价铬","2021-11-02",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[106,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","总银","2021-11-02",0,null,null,"<0.00004",0.5,null,"mg/L","否",null,null,"是"]
[107,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","挥发酚","2021-11-02",0,null,null,"<0.01",1,null,"mg/L","否",null,null,"是"]
[108,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","氰化物（总氰化合物）","2021-11-02",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[109,"阳西县中医院","专科医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水排放口(DW001)","氨氮（NH3-N）","2021-11-02",0,null,null,10.6,15,null,"mg/L","否",null,null,"是"]
[110,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","五日生化需氧量","2021-09-26",0,null,null,5.2,10,null,"mg/L","否",null,null,"是"]
[111,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","动植物油","2021-09-26",0,null,null,0.12,1,null,"mg/L","否",null,null,"是"]
[112,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","氨氮（NH3-N）","2021-09-26",0,null,null,0.442,"5;8",null,"mg/L","否",null,null,"是"]
[113,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","pH值","2021-09-26",0,null,null,6.91,9,6,"无量纲","否",null,null,"是"]
[114,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","六价铬","2021-09-26",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
[115,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水总排放口(DW001)","总磷（以P计）","2021-09-26",0,null,null,0.18,0.5,null,"mg/L","否",null,null,"是"]
[116,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铬","2021-09-26",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
[117,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铅","2021-09-26",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
[118,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","色度","2021-09-26",0,null,null,2,30,null,"倍","否",null,null,"是"]
[119,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","悬浮物","2021-09-26",0,null,null,"<4",10,null,"mg/L","否",null,null,"是"]
[120,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","阴离子表面活性剂","2021-09-26",0,null,null,"<0.05",0.5,null,"mg/L","否",null,null,"是"]
[121,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总氮（以N计）","2021-09-26",0,null,null,8.84,15,null,"mg/L","否",null,null,"是"]
[122,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","石油类","2021-09-26",0,null,null,"<0.06",1,null,"mg/L","否",null,null,"是"]
[123,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总镉","2021-09-26",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
[124,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","废水总排放口(DW001)","化学需氧量","2021-09-26",0,null,null,20,40,null,"mg/L","否",null,null,"是"]
[125,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总砷","2021-09-26",0,null,null,0.0008,0.1,null,"mg/L","否",null,null,"是"]
[126,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总汞","2021-09-26",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
[127,"阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","烷基汞","2021-09-26",0,null,null,0,0,null,"mg/L","否",null,null,"是"]
[128,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,纺织染整工业","废水处理后排放口(DW001)","化学需氧量","2021-04-23",0,null,9310,27,260,null,"mg/L","否",null,null,"是"]
[129,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,A级","废水处理后排放口(DW001)","总氮（以N计）","2021-04-23",0,null,372,10.2,35,null,"mg/L","否",null,null,"是"]
[130,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水处理后排放口(DW001)","pH值","2021-04-23",0,null,7.2,7.2,9,6,"无量纲","否",null,null,"是"]
[131,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,合成氨工业","废水处理后排放口(DW001)","氨氮（NH3-N）","2021-04-23",0,null,71.3,1.45,30,null,"mg/L","否",null,null,"是"]
[132,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水处理后排放口(DW001)","动植物油","2021-04-23",0,null,47.1,1.02,100,null,"mg/L","否",null,null,"是"]
[133,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水处理后排放口(DW001)","悬浮物","2021-04-23",0,null,2370,8,230,null,"mg/L","否",null,null,"是"]
[134,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,B级","废水处理后排放口(DW001)","总磷（以P计）","2021-04-23",0,null,138,0.57,4,null,"mg/L","否",null,null,"是"]
[135,"阳江市平海制品有限公司","鱼糜制品及水产品干腌制加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,天然橡胶乳加工、酒精、味精、皮革、化纤浆粕工业","废水处理后排放口(DW001)","五日生化需氧量","2021-04-23",0,null,2560,7.4,150,null,"mg/L","否",null,null,"是"]
[136,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","总磷（以P计）","2021-03-10",0,null,null,0.09,2,null,"mg/L","否",null,null,"是"]
[137,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","废水处理后出口(DW001)","五日生化需氧量","2021-03-10",0,null,null,17.9,150,null,"mg/L","否",null,null,"是"]
[138,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,一切排污单位","废水处理后出口(DW001)","动植物油","2021-03-10",0,null,null,0.35,100,null,"mg/L","否",null,null,"是"]
[139,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","化学需氧量","2021-03-10",0,null,null,65,200,null,"mg/L","否",null,null,"是"]
[140,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","氨氮（NH3-N）","2021-03-10",0,null,null,1.88,15,null,"mg/L","否",null,null,"是"]
[141,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","石油类","2021-03-10",0,null,null,0.79,10,null,"mg/L","否",null,null,"是"]
[142,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口(DW001)","六价铬","2021-03-10",0,null,null,0.022,0.25,null,"mg/L","否",null,null,"是"]
[143,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","悬浮物","2021-03-10",0,null,null,16,100,null,"mg/L","否",null,null,"是"]
[144,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口(DW001)","总镍","2021-03-10",0,null,null,"<0.005",0.5,null,"mg/L","否",null,null,"是"]
[145,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口(DW001)","总铬","2021-03-10",0,null,null,"<0.03",0.75,null,"mg/L","否",null,null,"是"]
[146,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,一切排污单位","废水处理后出口(DW001)","pH值","2021-03-10",0,null,null,7.7,9,6,"无量纲","否",null,null,"是"]
[147,"阳江开宝新材料实业有限公司","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口(DW001)","总氮（以N计）","2021-03-10",0,null,null,10.8,35,null,"mg/L","否",null,null,"是"]
[148,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","总余氯","2021-09-27",0,null,null,0.31,null,null,"mg/L","否",null,null,"否"]
[149,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","挥发酚","2021-09-27",0,null,null,"<0.01",1,null,"mg/L","否",null,null,"是"]
[150,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","色度","2021-09-27",0,null,null,2,null,null,"倍","否",null,null,"否"]
[151,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","化学需氧量","2021-09-27",0,null,null,21,250,null,"mg/L","否",null,null,"是"]
[152,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","粪大肠菌群","2021-09-27",0,null,null,"<20",5000,null,"个/L","否",null,null,"是"]
[153,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","pH值","2021-09-27",0,null,null,6.93,9,6,"无量纲","否",null,null,"是"]
[154,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","悬浮物","2021-09-27",0,null,null,5,60,null,"mg/L","否",null,null,"是"]
[155,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","五日生化需氧量","2021-09-27",0,null,null,5.4,100,null,"mg/L","否",null,null,"是"]
[156,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","石油类","2021-09-27",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[157,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","氰化物（总氰化合物）","2021-09-27",0,null,null,"<0.004",0.5,null,"mg/L","否",null,null,"是"]
[158,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","动植物油","2021-09-27",0,null,null,"<0.06",20,null,"mg/L","否",null,null,"是"]
[159,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","阴离子表面活性剂（LAS）","2021-09-27",0,null,null,0.16,10,null,"mg/L","否",null,null,"是"]
[160,"阳东区人民医院","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口(DW001)","氨氮（NH3-N）","2021-09-27",0,null,null,5.8,null,null,"mg/L","否",null,null,"否"]
[161,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,车间生产设施废水排放口","总排放口(DW004)","六价铬","2021-03-02",0,null,null,0.004,0.1,null,"mg/L","否",null,null,"是"]
[162,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","总磷（以P计）","2021-03-02",0,null,null,0.03,1,null,"mg/L","否",null,null,"是"]
[163,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","化学需氧量","2021-03-02",0,null,null,48,100,null,"mg/L","否",null,null,"是"]
[164,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","氨氮（NH3-N）","2021-03-02",0,null,null,19.3,25,null,"mg/L","否",null,null,"是"]
[165,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","pH值","2021-03-02",0,null,null,7.82,9,6,"无量纲","否",null,null,"是"]
[166,"阳西县长江制革有限公司","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,车间生产设施废水排放口","总排放口(DW004)","总铬","2021-03-02",0,null,null,"<0.03",1.5,null,"mg/L","否",null,null,"是"]
[167,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","排放口(1)","化学需氧量","2021-09-26",0,null,null,10,40,null,"mg/L","否",null,null,"是"]
[168,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","总氮（以N计）","2021-09-26",0,null,null,5.68,20,null,"mg/L","否",null,null,"是"]
[169,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","阴离子表面活性剂","2021-09-26",0,null,null,"<0.05",1,null,"mg/L","否",null,null,"是"]
[170,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铅","2021-09-26",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
[171,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总汞","2021-09-26",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
[172,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","色度","2021-09-26",0,null,null,2,30,null,"倍","否",null,null,"是"]
[173,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","烷基汞","2021-09-26",0,null,null,"<0.00001",0,null,"mg/L","否",null,null,"是"]
[174,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","动植物油","2021-09-26",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
[175,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","五日生化需氧量","2021-09-26",0,null,null,3.3,20,null,"mg/L","否",null,null,"是"]
[176,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","悬浮物","2021-09-26",0,null,null,6,20,null,"mg/L","否",null,null,"是"]
[177,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铬","2021-09-26",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
[178,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","六价铬","2021-09-26",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
[179,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","pH值","2021-09-26",0,null,null,6.93,9,6,"无量纲","否",null,null,"是"]
[180,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总镉","2021-09-26",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
[181,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","石油类","2021-09-26",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
[182,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总砷","2021-09-26",0,null,null,"<0.0003",0.1,null,"mg/L","否",null,null,"是"]
[183,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2005年12月31日前建设","排放口(1)","总磷（以P计）","2021-09-26",0,null,null,0.22,0.5,null,"mg/L","否",null,null,"是"]
[184,"阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","氨氮（NH3-N）","2021-09-26",0,null,null,0.082,"5;8",null,"mg/L","否",null,null,"是"]
[185,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","废水总排口(1)","化学需氧量","2021-09-27",0,null,null,36,40,null,"mg/L","否",null,null,"是"]
[186,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","总氮（以N计）","2021-09-27",0,null,null,12.7,20,null,"mg/L","否",null,null,"是"]
[187,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","阴离子表面活性剂","2021-09-27",0,null,null,"<0.05",1,null,"mg/L","否",null,null,"是"]
[188,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总铅","2021-09-27",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
[189,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总汞","2021-09-27",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
[190,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","色度","2021-09-27",0,null,null,2,30,null,"倍","否",null,null,"是"]
[191,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","废水总排口(1)","总磷（以P计）","2021-09-27",0,null,null,0.72,1,null,"mg/L","否",null,null,"是"]
[192,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","烷基汞","2021-09-27",0,null,null,0,0,null,"mg/L","否",null,null,"是"]
[193,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","动植物油","2021-09-27",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
[194,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","五日生化需氧量","2021-09-27",0,null,null,10,20,null,"mg/L","否",null,null,"是"]
[195,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","悬浮物","2021-09-27",0,null,null,7,20,null,"mg/L","否",null,null,"是"]
[196,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总铬","2021-09-27",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
[197,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","六价铬","2021-09-27",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
[198,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","pH值","2021-09-27",0,null,null,7.04,9,6,"无量纲","否",null,null,"是"]
[199,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总镉","2021-09-27",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
[200,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","石油类","2021-09-27",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
[201,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总砷","2021-09-27",0,null,null,0.0007,0.1,null,"mg/L","否",null,null,"是"]
[202,"阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","B标准","废水总排口(1)","氨氮（NH3-N）","2021-09-27",0,null,null,6.1,8,null,"mg/L","否",null,null,"是"]
[203,"东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","化学需氧量","2021-12-01",0,null,null,5,100,null,"mg/L","否",null,null,"是"]
[204,"东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","总磷（以P计）","2021-12-01",0,null,null,0.02,3,null,"mg/L","否",null,null,"是"]
[205,"东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","总铬","2021-12-01",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
[206,"东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","氨氮（NH3-N）","2021-12-01",0,null,null,2.27,25,null,"mg/L","否",null,null,"是"]
[207,"东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物特别排放限值","总排放口(DW001)","六价铬","2021-12-01",0,null,null,0.009,0.05,null,"mg/L","否",null,null,"是"]
[208,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","悬浮物","2021-03-11",0,null,283,8,60,null,"mg/L","否",null,null,"是"]
[209,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水处理后排放口(1)","pH值","2021-03-11",0,null,6.5,7.5,9,6,"mg/L","否",null,null,"是"]
[210,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水处理后排放口(1)","动植物油","2021-03-11",0,null,1.59,1.04,10,null,"mg/L","否",null,null,"是"]
[211,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","五日生化需氧量","2021-03-11",0,null,1370,1.9,20,null,"mg/L","否",null,null,"是"]
[212,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","氨氮（NH3-N）","2021-03-11",0,null,34.7,0.152,10,null,"mg/L","否",null,null,"是"]
[213,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","石油类","2021-03-11",0,null,1.1,0.6,5,null,"mg/L","否",null,null,"是"]
[214,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","化学需氧量","2021-03-11",0,null,4970,7,90,null,"mg/L","否",null,null,"是"]
[215,"嘉吉粮油（阳江）有限公司","食用植物油加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水处理后排放口(1)","磷酸盐（以P计）","2021-03-11",0,null,28.2,0.1,0.5,null,"mg/L","否",null,null,"是"]
[216,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水处理后出口(J2021030128-1-2-001)","悬浮物","2021-03-10",0,null,78,75,100,null,"mg/L","否",null,null,"是"]
[217,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水处理后出口(J2021030128-1-2-001)","氨氮（NH3-N）","2021-03-10",0,null,6.57,5.34,15,null,"mg/L","否",null,null,"是"]
[218,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水处理后出口(J2021030128-1-2-001)","化学需氧量","2021-03-10",0,null,334,180,110,null,"mg/L","是",0.64,null,"是"]
[219,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","废水处理后出口(J2021030128-1-2-001)","pH值","2021-03-10",0,null,5.9,8.9,9,6,"无量纲","否",null,null,"是"]
[220,"阳江市皇玛服饰有限公司","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,三级标准,2005年12月31日前建设","废水处理后出口(J2021030128-1-2-001)","总磷（以P计）","2021-03-10",0,null,1.66,0.19,4,null,"mg/L","否",null,null,"是"]
[221,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水处理后出口(J2021030128-1-2-001)","五日生化需氧量","2021-03-10",0,null,91.9,49.5,30,null,"mg/L","是",0.65,null,"是"]
[222,"阳江市皇玛服饰有限公司","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","废水处理后出口(J2021030128-1-2-001)","动植物油","2021-03-10",0,null,1.87,0.61,15,null,"mg/L","否",null,null,"是"]
[223,"阳江市皇玛服饰有限公司","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理后出口(J2021030128-1-2-001)","总氮（以N计）","2021-03-10",0,null,12.2,6.06,35,null,"mg/L","否",null,null,"是"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}