{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":71,"n_cols":18,"rows_kept":71,"merged":[[0,0,0,17]],"flags":["formulas_cached_only"]}
["附件3：阳江市2021年重点监控企业污染源（污水处理厂）监督性监测结果"]
["企业名称","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","流量(m³/s)","水温(°C)","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","总排放口(DW001)","总磷（以P计）","2021-01-06",0,null,1.24,0.08,0.5,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","总氮（以N计）","2021-01-06",0,null,23.1,8.75,15,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","悬浮物","2021-01-06",0,null,83,4,10,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(DW001)","氨氮（NH3-N）","2021-01-06",0,20,17.2,0.429,"5;8",null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","总排放口(1)","氨氮（NH3-N）","2021-04-06",0,25,35.1,0.589,5,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","悬浮物","2021-04-06",0,null,104,7,10,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","总氮（以N计）","2021-04-06",0,null,40.5,4.54,15,null,"mg/L","否",null,null,"是"]
["阳西捷晖净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","总排放口(1)","总磷（以P计）","2021-04-06",0,null,5.12,0.11,0.5,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","总氮（以N计）","2021-01-06",0,null,37.5,5.64,20,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","氨氮（NH3-N）","2021-01-06",0,20,31.5,2.38,"8;15",null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","排放口","总磷（以P计）","2021-01-06",0,null,6.27,0.73,1,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","悬浮物","2021-01-06",0,null,65,8,20,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","氨氮（NH3-N）","2021-04-06",0,25,52.8,0.463,"8;15",null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","悬浮物","2021-04-06",0,null,63,6,20,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","排放口(DW001)","总磷（以P计）","2021-04-06",0,null,5.26,0.7,1,null,"mg/L","否",null,null,"是"]
["阳西中炬水务有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(DW001)","总氮（以N计）","2021-04-06",0,null,57.1,8.68,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","五日生化需氧量","2021-09-26",0,null,null,5.2,10,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","动植物油","2021-09-26",0,null,null,0.12,1,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","氨氮（NH3-N）","2021-09-26",0,null,null,0.442,"5;8",null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","pH值","2021-09-26",0,null,null,6.91,9,6,"无量纲","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","六价铬","2021-09-26",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水总排放口(DW001)","总磷（以P计）","2021-09-26",0,null,null,0.18,0.5,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铬","2021-09-26",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铅","2021-09-26",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","色度","2021-09-26",0,null,null,2,30,null,"倍","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","悬浮物","2021-09-26",0,null,null,"<4",10,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","阴离子表面活性剂","2021-09-26",0,null,null,"<0.05",0.5,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总氮（以N计）","2021-09-26",0,null,null,8.84,15,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","石油类","2021-09-26",0,null,null,"<0.06",1,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总镉","2021-09-26",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总砷","2021-09-26",0,null,null,0.0008,0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总汞","2021-09-26",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
["阳江市阳东迅捷水质净化有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","烷基汞","2021-09-26",0,null,null,0,0,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","总氮（以N计）","2021-09-26",0,null,null,5.68,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","阴离子表面活性剂","2021-09-26",0,null,null,"<0.05",1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铅","2021-09-26",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总汞","2021-09-26",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","色度","2021-09-26",0,null,null,2,30,null,"倍","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","烷基汞","2021-09-26",0,null,null,"<0.00001",0,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","动植物油","2021-09-26",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","五日生化需氧量","2021-09-26",0,null,null,3.3,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","悬浮物","2021-09-26",0,null,null,6,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铬","2021-09-26",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","六价铬","2021-09-26",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","pH值","2021-09-26",0,null,null,6.93,9,6,"无量纲","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总镉","2021-09-26",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","石油类","2021-09-26",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总砷","2021-09-26",0,null,null,"<0.0003",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2005年12月31日前建设","排放口(1)","总磷（以P计）","2021-09-26",0,null,null,0.22,0.5,null,"mg/L","否",null,null,"是"]
["阳江市阳东区森禾净水有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","氨氮（NH3-N）","2021-09-26",0,null,null,0.082,"5;8",null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","总氮（以N计）","2021-09-27",0,null,null,12.7,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","阴离子表面活性剂","2021-09-27",0,null,null,"<0.05",1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总铅","2021-09-27",0,null,null,"<0.001",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总汞","2021-09-27",0,null,null,"<0.00004",0.001,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","色度","2021-09-27",0,null,null,2,30,null,"倍","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","废水总排口(1)","总磷（以P计）","2021-09-27",0,null,null,0.72,1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","烷基汞","2021-09-27",0,null,null,0,0,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","动植物油","2021-09-27",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","五日生化需氧量","2021-09-27",0,null,null,10,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","悬浮物","2021-09-27",0,null,null,7,20,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总铬","2021-09-27",0,null,null,"<0.03",0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","六价铬","2021-09-27",0,null,null,"<0.004",0.05,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","pH值","2021-09-27",0,null,null,7.04,9,6,"无量纲","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总镉","2021-09-27",0,null,null,"<0.0001",0.01,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口(1)","石油类","2021-09-27",0,null,null,"<0.06",3,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口(1)","总砷","2021-09-27",0,null,null,0.0007,0.1,null,"mg/L","否",null,null,"是"]
["阳江市阳东区鑫泰源污水处理有限公司","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","B标准","废水总排口(1)","氨氮（NH3-N）","2021-09-27",0,null,null,6.1,8,null,"mg/L","否",null,null,"是"]
["阳江市皇玛服饰有限公司","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,三级标准,2005年12月31日前建设","废水处理后出口(J2021030128-1-2-001)","总磷（以P计）","2021-03-10",0,null,1.66,0.19,4,null,"mg/L","否",null,null,"是"]
["阳江市皇玛服饰有限公司","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理后出口(J2021030128-1-2-001)","总氮（以N计）","2021-03-10",0,null,12.2,6.06,35,null,"mg/L","否",null,null,"是"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}