{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["废气排放","废水排放","无组织","周边环境","厂界噪声"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废气排放","index":0,"n_rows":97,"n_cols":18,"rows_kept":97,"merged":[[1,0,27,0],[1,1,4,1],[5,1,7,1],[8,1,11,1],[12,1,14,1],[15,1,18,1],[19,1,24,1],[25,1,27,1],[28,0,75,0],[28,1,30,1],[31,1,39,1],[40,1,49,1],[50,1,53,1],[54,1,58,1],[59,1,61,1],[62,1,63,1],[65,1,69,1],[70,1,75,1],[76,0,96,0],[76,1,85,1],[86,1,88,1],[89,1,92,1],[93,1,96,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","实测浓度","折算浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2022年阳春分局执法监测","广东春潭水泥制造有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,破碎机、磨机、包装机及其他通风生产设备","1#窑头烟囱029(DA029)","颗粒物","2022-06-28","0","0","10","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","广东春潭水泥制造有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表1）现有与新建企业大气污染物排放限值,水泥制造,水泥窑及窑尾余热利用系统","1#窑尾烟囱028(DA028)","氮氧化物","2022-06-28","196","152","400","","mg/m3","否","","","是"]
["2022年执法监测","广东春潭水泥制造有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","1#窑尾烟囱028(DA028)","颗粒物","2022-06-28","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","广东春潭水泥制造有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","1#窑尾烟囱028(DA028)","二氧化硫","2022-06-28","38","29","100","","mg/m3","否","","","是"]
["2022年执法监测","广东金水晶玻璃股份有限公司","大气环境","日用玻璃制品制造","广东省玻璃工业大气污染物排放标准(DB44/2159-2019)","表1 大气污染物排放限值,平板玻璃,玻璃熔窑","电助熔炉烟气排放口001(DA001)","二氧化硫","2022-11-04","0","0","280","","mg/m3","否","","低于检出限3mg/m3","是"]
["2022年执法监测","广东金水晶玻璃股份有限公司","大气环境","日用玻璃制品制造","广东省玻璃工业大气污染物排放标准(DB44/2159-2019)","表1 大气污染物排放限值,平板玻璃,玻璃熔窑","电助熔炉烟气排放口001(DA001)","颗粒物","2022-11-04","0","0","30","","mg/m3","否","","低于方法检出限20mg/m3","是"]
["2022年执法监测","广东金水晶玻璃股份有限公司","大气环境","日用玻璃制品制造","广东省玻璃工业大气污染物排放标准(DB44/2159-2019)","表1 大气污染物排放限值,平板玻璃,玻璃熔窑","电助熔炉烟气排放口001(DA001)","氮氧化物（以NO2计）","2022-11-04","88","168","550","","mg/m3","否","","","是"]
["2022年执法监测","华润水泥（阳春）有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,破碎机、磨机、包装机及其他通风生产设备","窑头002(DA002)","颗粒物","2022-10-25","0","0","10","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","华润水泥（阳春）有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","废气监测点001(DA001)","氮氧化物","2022-10-25","226","175","320","","mg/m3","否","","","是"]
["2022年执法监测","华润水泥（阳春）有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","废气监测点001(DA001)","二氧化硫","2022-10-25","11","9","100","","mg/m3","否","","","是"]
["2022年执法监测","华润水泥（阳春）有限公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","废气监测点001(DA001)","颗粒物","2022-10-25","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","广东新兴铸管有限公司","大气环境","黑色金属铸造","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","烧结机头废气处理后排放口001(DA001)","颗粒物","2022-04-21","0","0","40","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","广东新兴铸管有限公司","大气环境","黑色金属铸造","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","烧结机头废气处理后排放口001(DA001)","氮氧化物","2022-04-21","25","13","300","","mg/m3","否","","","是"]
["2022年执法监测","广东新兴铸管有限公司","大气环境","黑色金属铸造","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机机尾带式焙烧机机尾其他生产设备","烧结机尾废气处理后排放口002(DA002)","颗粒物","2022-04-21","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","阳春海螺水泥有限责任公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","2#窑尾烟囱431(DA431)","颗粒物","2022-06-23","25","18","20","","mg/m3","否","","","是"]
["2022年执法监测","阳春海螺水泥有限责任公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","2#窑尾烟囱431(DA431)","氮氧化物","2022-06-23","221","161","320","","mg/m3","否","","","是"]
["2022年执法监测","阳春海螺水泥有限责任公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","2#窑尾烟囱431(DA431)","二氧化硫","2022-06-23","27","20","100","","mg/m3","否","","","是"]
["2022年执法监测","阳春海螺水泥有限责任公司","大气环境","水泥制造","水泥工业大气污染物排放标准(GB4915-2013)","（表2）大气污染物特别排放限值,水泥制造,水泥窑及窑尾余热利用系统","2#窑头烟囱433(DA433)","颗粒物","2022-06-23","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机机尾带式焙烧机机尾其他生产设备","1#烧结机尾废气排放口010(DA010)","颗粒物","2022-06-29","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机机尾带式焙烧机机尾其他生产设备","2#烧结机尾废气排放口013(DA013)","颗粒物","2022-06-29","0","0","20","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","2#烧结机头废气排放口012(DA012)","颗粒物","2022-06-29","22","18","40","","mg/m3","否","","","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","2#烧结机头废气排放口012(DA012)","氮氧化物","2022-06-29","36","29","300","","mg/m3","否","","","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","1#烧结机头废气排放口009(DA009)","颗粒物","2022-06-29","0","0","40","","mg/m3","否","","低于检出限20mg/m3","是"]
["2022年执法监测","阳春新钢铁有限责任公司","大气环境","黑色金属冶炼和压延加工业 ","钢铁烧结、球团工业大气污染物排放标准(GB28662-2012)","（表3）大气污染物特别排放限值,烧结机球团焙烧设备","1#烧结机头废气排放口009(DA009)","氮氧化物","2022-06-29","44","36","300","","mg/m3","否","","","是"]
["2022年执法监测","阳春市威利邦木业有限公司","大气环境","纤维板制造","广东省大气污染物排放限值(DB4427-2001)","颗粒物","排放口(DA001)","颗粒物","2022-10-27","32","32","120","","mg/m3","否","","根据文件要求，该工艺不用只测实测浓度，不用折算。","是"]
["2022年执法监测","阳春市威利邦木业有限公司","大气环境","纤维板制造","广东省大气污染物排放限值标准 （完整）(DB44/27—2001)","表2   工艺废气大气污染物排放限值（第二时段） ,最高允许排放浓度,氮氧化物,氮氧化物（硝酸、氮肥和火炸药生产）","排放口(DA001)","氮氧化物","2022-10-27","62","62","120","","mg/m3","否","","","是"]
["2022年执法监测","阳春市威利邦木业有限公司","大气环境","纤维板制造","广东省大气污染物排放限值标准 （完整）(DB44/27—2001)","表2   工艺废气大气污染物排放限值（第二时段） ,最高允许排放浓度,二氧化硫,二氧化硫（其它）","排放口(DA001)","二氧化硫","2022-10-27","0","0","500","","mg/m3","否","","低于检出限3mg/m3","是"]
["2022年阳东区执法监测","阳江市阳东区合和新型墙体建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱001(DA001)","二氧化硫","2022-06-29","23","98","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区合和新型墙体建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱001(DA001)","氮氧化物","2022-06-29","28","119","200","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区合和新型墙体建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","广东省大气污染物排放限值标准 （完整）(DB44/27—2001)","表5 锅炉大气污染物最高允许排放限值,燃煤锅炉,第二时段,二类区域：其它锅炉","窑烟囱001(DA001)","烟尘","2022-06-29","<20","<20","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口3#","苯","2022-07-03","0.04","0.04","1","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口3#","总VOCs","2022-07-03","3.86","3.86","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口3#","甲苯和二甲苯合计","2022-07-03","0.50","0.50","20","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口1#","总VOCs","2022-07-03","3.56","3.56","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口1#","甲苯和二甲苯合计","2022-07-03","0.49","0.49","20","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口1#","苯","2022-07-03","0.03","0.03","1","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口2#","总VOCs","2022-07-03","4.37","4.37","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口2#","甲苯和二甲苯合计","2022-07-03","0.66","0.66","20","","mg/m3","否","","","是"]
["2022年阳东区执法监测","广东木森日用品有限公司阳江市阳东万象三分公司","大气环境","木质家具制造","家具制造行业挥发性有机化合物排放标准[地标](DB44/814-2010)","表１ 排气筒VOCs排放限值,最高允许排放浓度,Ⅱ时段","油漆车间排放口2#","苯","2022-07-03","0.02","0.02","1","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","《大气污染物排放限值》（DB44/27-2001）(DB44/27-2001)","总VOCs","三期车间上胶染色工序废气排放口1","总VOCs","2022-07-01","5.45","5.45","","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","三期车间上胶染色工序废气排放口1","臭气浓度","2022-07-01","229","229","","","无量纲","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","擦布车间废气排放口","臭气浓度","2022-07-01","309","309","","","无量纲","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","《大气污染物排放限值》（DB44/27-2001）(DB44/27-2001)","总VOCs","擦布车间废气排放口","总VOCs","2022-07-01","4.87","4.87","","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","清洁抛车间废气排放口","臭气浓度","2022-07-01","174","174","","","无量纲","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","《大气污染物排放限值》（DB44/27-2001）(DB44/27-2001)","总VOCs","清洁抛车间废气排放口","总VOCs","2022-07-01","6.42","6.42","","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","《大气污染物排放限值》（DB44/27-2001）(DB44/27-2001)","总VOCs","尼龙车间废气排放口","总VOCs","2022-07-01","6.57","6.57","","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","尼龙车间废气排放口","臭气浓度","2022-07-01","309","309","","","无量纲","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表2）恶臭污染物排放标准值,排气筒高度15m","三期车间上胶染色工序废气排放口2","臭气浓度","2022-07-01","229","229","","","无量纲","否","","","否"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","《大气污染物排放限值》（DB44/27-2001）(DB44/27-2001)","总VOCs","三期车间上胶染色工序废气排放口2","总VOCs","2022-07-01","7.42","7.42","","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江嘉合化工有限公司","大气环境","有机化学原料制造","","","尾气处理1001(DA001)","甲醇","2022-06-24","<2","<2","50","","mg/Nm3","否","","监测口过小无法测量工况","否"]
["2022年阳东区执法监测","阳江嘉合化工有限公司","大气环境","有机化学原料制造","","","尾气处理1001(DA001)","挥发性有机物","2022-06-24","3.15","3.15","","","mg/L","否","","监测口过小无法测量工况","否"]
["2022年阳东区执法监测","阳江嘉合化工有限公司","大气环境","有机化学原料制造","石油化学工业污染物排放标准(GB31571-2015)","（表5）大气污染物特别排放限值,废水处理有机废气收集处理装置焚烧类有机排放口","尾气处理1001(DA001)","非甲烷总烃","2022-06-24","25.6","25.6","120","","mg/m3","否","","监测口过小无法测量工况","否"]
["2022年阳东区执法监测","阳江嘉合化工有限公司","大气环境","有机化学原料制造","","","尾气处理1001(DA001)","甲醛","2022-06-24","0.04","0.04","5","","mg/Nm3","否","","监测口过小无法测量工况","否"]
["2022年阳东区执法监测","阳江市天力冷却塔有限公司","大气环境","金属结构制造","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,涂层机组","1号油漆排放口","甲苯","2022-06-28","0.01","0.01","40","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市天力冷却塔有限公司","大气环境","金属结构制造","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,涂层机组","1号油漆排放口","二甲苯（总量）","2022-06-28","0.94","0.94","40","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市天力冷却塔有限公司","大气环境","金属结构制造","大气污染物排放限值[地标]DB44/27-2001(DB44/27-2001)","总挥发性有机物","1号油漆排放口","总挥发性有机物","2022-06-28","12.2","12.2","","","mg/Nm3","否","","","否"]
["2022年阳东区执法监测","阳江市天力冷却塔有限公司","大气环境","金属结构制造","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,拉矫、精整、抛丸、修磨、焊接机及其他生产设施","1号油漆排放口","颗粒物","2022-06-28","<20","<20","20","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市天力冷却塔有限公司","大气环境","金属结构制造","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,涂层机组","1号油漆排放口","苯","2022-06-28","7.61","7.61","8.0","","mg/m3","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱1#001(DA001)","颗粒物","2022-06-22","20.6","26.0","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱1#001(DA001)","氮氧化物","2022-06-22","6","8","200","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱1#001(DA001)","二氧化硫","2022-06-22","6","7","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱001(DA001)","二氧化硫","2022-06-23","42","60","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","窑烟囱001(DA001)","氮氧化物","2022-06-23","4","6","200","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表1在用锅炉大气污染物排放浓度限值（珠三角地区）,燃生物质成型燃料锅炉","锅炉废气排放口DA001","颗粒物","2022-06-15","<20","<20","20","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","电炉排放口DA016(DA016)","氮氧化物","2022-07-01","7","7","300","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,酸洗机组","电炉排放口DA016(DA016)","硝酸雾","2022-07-01","<0.7","<0.7","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","电炉排放口DA016(DA016)","二氧化硫","2022-07-01","13","13","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,涂层机组","电炉排放口DA016(DA016)","非甲烷总烃","2022-07-01","2.15","2.15","80","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","轧钢工业大气污染物排放标准(GB28665-2012)","（表1、表2）现有和新建企业有组织大气污染物排放浓度限值,热处理炉","电炉排放口DA016(DA016)","颗粒物","2022-07-01","<20","<20","20","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","1#窑烟囱001(DA001)","氮氧化物","2022-06-22","48","48","200","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","1#窑烟囱001(DA001)","颗粒物","2022-06-22","11.2","11.2","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","1#窑烟囱001(DA001)","二氧化硫","2022-06-22","75","75","150","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","2#窑烟囱002(DA002)","颗粒物","2022-06-22","10.4","10.4","30","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表1、表2）现有和新建企业大气污染物排放浓度限值,人工干燥及焙烧","2#窑烟囱002(DA002)","氮氧化物","2022-06-22","73","73","200","","mg/m3","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（修改单）新建企业大气污染物排放浓度限值,人工干燥及焙烧","2#窑烟囱002(DA002)","二氧化硫","2022-06-22","81","81","150","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","6废气排放口(DA001)","烟气黑度（林格曼黑度，级）","2022-10-18","<1","<1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","6废气排放口(DA001)","汞及其化合物","2022-10-18","0.0155","0.0159","0.03","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","5废气排放口(DA001)","烟气黑度（林格曼黑度，级）","2022-10-18","<1","<1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","5废气排放口(DA001)","汞及其化合物","2022-10-18","0.0146","0.0160","0.03","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表2）大气污染物特别排放限值,烟囱或烟道,燃煤锅炉","1废气排放口(DA001)","汞及其化合物","2022-12-16","0.0104","0.0124","0.03","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","1废气排放口(DA001)","烟气黑度（林格曼黑度，级）","2022-12-16","<1","<1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","3废气排放口(DA001)","烟气黑度（林格曼黑度，级）","2022-12-16","<1","<1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","3废气排放口(DA001)","汞及其化合物","2022-12-16","0.0115","0.0131","0.03","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱排放口,燃煤锅炉，以油、气体为燃料的锅炉或燃汽轮机组","2废气排放口(DA001)","烟气黑度（林格曼黑度，级）","2022-12-16","<1","<1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西海滨电力发展有限公司","大气环境","火力发电","火电厂大气污染物排放标准(GB13223-2011)","（表1）火力发电锅炉及燃汽轮机组大气污染物排放浓度限值,烟囱或烟道,燃煤锅炉,全部,通用","2废气排放口(DA001)","汞及其化合物","2022-12-16","0.0095","0.0112","0.03","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","建华建材（阳江）有限公司","大气环境","砼结构构件制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃煤锅炉","锅炉废气排放口001(DA001)","二氧化硫","2022-05-13","22","54","200","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","建华建材（阳江）有限公司","大气环境","砼结构构件制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃煤锅炉","锅炉废气排放口001(DA001)","颗粒物","2022-05-13","<20","28","30","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","建华建材（阳江）有限公司","大气环境","砼结构构件制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃煤锅炉","锅炉废气排放口001(DA001)","氮氧化物","2022-05-13","74","181","200","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西美味鲜食品有限公司","水环境","酱油、食醋及类似制品制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃气锅炉","废气排放口(DA001)","氮氧化物","2022-11-01","34","45","150","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西美味鲜食品有限公司","水环境","酱油、食醋及类似制品制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃油锅炉","废气排放口(DA001)","颗粒物","2022-11-01","2.1","2.8","20","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西美味鲜食品有限公司","水环境","酱油、食醋及类似制品制造","广东省锅炉大气污染物排放标准[地标](DB44/765-2019)","表2新建锅炉大气污染物排放浓度限值,燃气锅炉","废气排放口(DA001)","二氧化硫","2022-11-01","<3","<3","50","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西美味鲜食品有限公司","水环境","酱油、食醋及类似制品制造","锅炉大气污染物排放标准(DB44/765-2010)","表1   锅炉烟尘最高允许排放浓度和烟气黑度限值,燃气锅炉,全部区域,烟气黑度 （2010年11月1日）","废气排放口(DA001)","烟气黑度","2022-11-01","<1","<1","1.0","","级","否","","","是"]
["2022年阳西分局执法监测","阳西博德精工建材有限公司","大气环境","建筑陶瓷制品制造","陶瓷工业污染物排放标准(GB25464-2010)","（表5）新建企业大气污染物排放浓度限值,喷雾干燥塔、陶瓷窑","废气排放口DA001(DA001)","颗粒物","2022-03-31","3.9","4.2","30","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西博德精工建材有限公司","大气环境","建筑陶瓷制品制造","陶瓷工业污染物排放标准(GB25464-2010)","（表4、表5）现有和新建企业大气污染物排放浓度限值,原料制备、干燥 喷雾干燥塔 水煤浆","废气排放口DA001(DA001)","氮氧化物","2022-03-31","57","61","180","","mg/m3","否","","","是"]
["2022年阳西分局执法监测","阳西博德精工建材有限公司","大气环境","建筑陶瓷制品制造","陶瓷工业污染物排放标准(GB25464-2010)","（表4、表5）现有和新建企业大气污染物排放浓度限值,烧成、烤花 辊道窑、隧道窑、梭式窑 油、气","废气排放口DA001(DA001)","林格曼黑度","2022-03-31","1","1","1","","级","否","","","是"]
["2022年阳西分局执法监测","阳西博德精工建材有限公司","大气环境","建筑陶瓷制品制造","陶瓷工业污染物排放标准(GB25464-2010)","（表5）新建企业大气污染物排放浓度限值,喷雾干燥塔、陶瓷窑","废气排放口DA001(DA001)","二氧化硫","2022-03-31","12","13","50","","mg/m3","否","","","是"]

{"sheet":"废水排放","index":1,"n_rows":344,"n_cols":18,"rows_kept":344,"merged":[[1,0,95,0],[1,1,5,1],[6,1,10,1],[11,1,15,1],[16,1,23,1],[24,1,30,1],[31,1,34,1],[35,1,37,1],[38,1,45,1],[46,1,50,1],[51,1,54,1],[55,1,57,1],[58,1,62,1],[63,1,67,1],[68,1,71,1],[72,1,76,1],[77,1,81,1],[82,1,85,1],[86,1,90,1],[91,1,95,1],[96,0,207,0],[96,1,101,1],[102,1,108,1],[109,1,121,1],[122,1,139,1],[140,1,143,1],[144,1,147,1],[148,1,165,1],[166,1,169,1],[170,1,174,1],[175,1,180,1],[181,1,189,1],[190,1,207,1],[208,0,278,0],[208,1,212,1],[213,1,221,1],[222,1,230,1],[231,1,237,1],[238,1,251,1],[252,1,260,1],[261,1,278,1],[279,0,343,0],[279,1,284,1],[285,1,290,1],[291,1,296,1],[297,1,302,1],[303,1,308,1],[309,1,314,1],[315,1,320,1],[321,1,326,1],[327,1,331,1],[332,1,337,1],[338,1,343,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","进口浓度","排放浓度","上限","下限","单位","是否超标","超标倍数","备注","是否有评价限值"]
["2022年阳春分局执法监测","阳春市碧源春环保科技有限公司（松柏镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口","总氮（以N计）","2022-01-18","46.8","4.22","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（松柏镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口","总磷（以P计）","2022-01-18","4.58","0.24","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（松柏镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口","氨氮（NH3-N）","2022-01-18","36.5","1.26","8","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（松柏镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口","pH值","2022-01-18","7.0","7.2","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（松柏镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口","化学需氧量","2022-01-18","203","10","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（双滘镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-19","12","1.47","8","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（双滘镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-19","34.6","4.75","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（双滘镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-19","4.54","0.22","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（双滘镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-19","7.0","7.6","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（双滘镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-19","109","7","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（八甲镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-19","109","11","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（八甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-19","7.3","7.7","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（八甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-19","3.89","0.08","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（八甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-19","31.6","1.12","8","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（八甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-19","52.9","5.56","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","阳春市春吉园区开发有限公司污水处理厂污水排放口001","pH值","2022-06-14","6.7","7.4","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","B标准","阳春市春吉园区开发有限公司污水处理厂污水排放口001","氨氮（NH3-N）","2022-06-14","2.37","1.11","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表3）选择控制项目最高允许排放浓度（日均值）","阳春市春吉园区开发有限公司污水处理厂污水排放口001","总镍","2022-06-14","0","0","0.05","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","阳春市春吉园区开发有限公司污水处理厂污水排放口001","总磷（以P计）","2022-06-14","0.4","0.03","1","","mg/L","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表3）选择控制项目最高允许排放浓度（日均值）","阳春市春吉园区开发有限公司污水处理厂污水排放口001","总铜","2022-06-14","0","0","0.5","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","阳春市春吉园区开发有限公司污水处理厂污水排放口001","悬浮物","2022-06-14","63","8","20","","mg/L","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","阳春市春吉园区开发有限公司污水处理厂污水排放口001","总氮（以N计）","2022-06-14","10.7","4.02","20","","mg/L","否","","","是"]
["2022年执法监测","阳春市春吉园区开发有限公司污水处理厂","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","阳春市春吉园区开发有限公司污水处理厂污水排放口001","化学需氧量","2022-06-14","62","15","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","化学需氧量","2022-06-14","","5","100","","mg/L","否","","","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","污水排放口(DW001)","总镍","2022-06-14","","0","1","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","污水排放口(DW001)","pH","2022-06-14","","6.8","9","6","mg/L","否","","","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","氨氮（NH3-N）","2022-06-14","","5.86","10","","mg/L","否","","","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","悬浮物","2022-06-14","","18","70","","mg/L","否","","","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,一切排污单位","污水排放口(DW001)","总铜","2022-06-14","","0","0.5","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市丰园污泥处理有限公司","水环境","有机肥料及微生物肥料制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,其他排污单位","污水排放口(DW001)","磷酸盐（以P计）","2022-06-14","","0.04","1","","mg/L","否","","","是"]
["2022年执法监测","阳春大洋扬翔农牧科技有限责任公司","水环境","猪的饲养","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","污水排放口(DW001)","pH值","2022-10-12","","6.9","9","6","mg/L","否","","","是"]
["2022年执法监测","阳春大洋扬翔农牧科技有限责任公司","水环境","猪的饲养","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,养殖、屠宰、肉制品加工","污水排放口(DW001)","化学需氧量","2022-10-12","","37","80","","mg/L","否","","","是"]
["2022年执法监测","阳春大洋扬翔农牧科技有限责任公司","水环境","猪的饲养","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","磷酸盐（以P计）","2022-10-12","","0.5","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春大洋扬翔农牧科技有限责任公司","水环境","猪的饲养","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","氨氮（NH3-N）","2022-10-12","","2.1","10","","mg/L","否","","","是"]
["2022年执法监测","阳春市维美纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","污水排放口","化学需氧量","2022-05-17","","73","90","","mg/L","否","","","是"]
["2022年执法监测","阳春市维美纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口","pH值","2022-05-17","","6.0","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市维美纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口","氨氮（NH3-N）","2022-05-17","","1.78","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表3）选择控制项目最高允许排放浓度（日均值）","排放口","总铜","2022-06-14","","0","0.5","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表3）选择控制项目最高允许排放浓度（日均值）","排放口","总镍","2022-06-14","","0","0.05","","mg/L","否","","低于检出限0.05mg/L","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","排放口","化学需氧量","2022-06-14","","20","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","总氮（以N计）","2022-06-14","","8.31","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","氨氮（NH3-N）","2022-06-14","","1.95","5;8","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","排放口","总磷（以P计）","2022-06-14","","0.2","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","悬浮物","2022-06-14","","7","10","","mg/L","否","","","是"]
["2022年执法监测","阳春市水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","pH值","2022-06-14","","6.7","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（河?镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-18","18.5","3.39","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（河?镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-18","7.7","8.2","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（河?镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-18","26","6","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（河?镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-18","12.2","1.51","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（河?镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-18","1.89","0.34","0.5","","mg/L","否","","","是"]
["2022年执法监测","广东省阳春酒厂有限公司","水环境","白酒制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","污水排放口001(DW001)","pH值","2022-06-14","","7.","9","6","mg/L","否","","","是"]
["2022年执法监测","广东省阳春酒厂有限公司","水环境","白酒制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","污水排放口001(DW001)","化学需氧量","2022-06-14","","10","90","","mg/L","否","","","是"]
["2022年执法监测","广东省阳春酒厂有限公司","水环境","白酒制造","发酵酒精和白酒工业水污染物排放标准(GB27631-2011)","现有和新建企业水污染物排放限值,企业废水总排放口,直接排放","污水排放口001(DW001)","悬浮物","2022-06-14","","13","50","","mg/L","否","","","是"]
["2022年执法监测","广东省阳春酒厂有限公司","水环境","白酒制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口001(DW001)","氨氮（NH3-N）","2022-06-14","","1.48","10","","mg/L","否","","","是"]
["2022年执法监测","阳春市长兴纸业有限公司","","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","污水排放口(DW001)","化学需氧量","2022-01-12","","37","90","","mg/L","否","","","是"]
["2022年执法监测","阳春市长兴纸业有限公司","","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口(DW001)","pH值","2022-01-12","","8.1","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市长兴纸业有限公司","","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口(DW001)","氨氮（NH3-N）","2022-01-12","","1.47","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（石望镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-18","7.6","8.1","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（石望镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-18","9.62","1.58","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（石望镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-18","49","10","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（石望镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-18","19.9","4.99","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（石望镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-18","1.24","0.36","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司 （河口镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-19","43.2","1.26","8","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司 （河口镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-19","5.49","0.07","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司 （河口镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-19","6.6","7.4","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司 （河口镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-19","168","5","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司 （河口镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-19","67.1","6.7","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市嘉和纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口(DW001)","pH值","2022-10-12","","7.1","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市嘉和纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口(DW001)","氨氮（NH3-N）","2022-10-12","","2.14","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市嘉和纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","污水排放口(DW001)","悬浮物","2022-10-12","","8","10","","mg/L","否","","","是"]
["2022年执法监测","阳春市嘉和纸业有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","污水排放口(DW001)","化学需氧量","2022-10-12","","86","90","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（圭岗镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,二级标准（水温＞12℃或≤12℃）,通用","污水排放口(DW001)","总氮（以N计）","2022-01-18","24","5.76","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（圭岗镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-18","7.3","7.4","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（圭岗镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-18","3.83","0.49","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（圭岗镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-18","18.4","1.38","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（圭岗镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-18","128","5","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（三甲镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-19","132","11","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（三甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-19","7.6","7.5","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（三甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-19","3.89","0.15","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（三甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-19","39.8","1.04","8","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（三甲镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-19","60.2","9.81","15","","mg/L","否","","","是"]
["2022年执法监测","广东安蒂丝纤维有限公司","","化纤织造及印染精加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,生物制药、皮革、苎麻脱胶、化纤浆粕、天然橡胶乳加工工业","污水排放口(DW001)","化学需氧量","2022-10-12","","97","100","","mg/L","否","","","是"]
["2022年执法监测","广东安蒂丝纤维有限公司","","化纤织造及印染精加工","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","污水排放口(DW001)","pH值","2022-10-12","","7.2","9","6","无量纲","否","","","是"]
["2022年执法监测","广东安蒂丝纤维有限公司","","化纤织造及印染精加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","氨氮（NH3-N）","2022-10-12","","4.35","10","","mg/L","否","","","是"]
["2022年执法监测","广东安蒂丝纤维有限公司","","化纤织造及印染精加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","污水排放口(DW001)","悬浮物","2022-10-12","","14","60","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（陂面镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-18","7.3","7.4","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（陂面镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-18","23.3","1.75","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（陂面镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-18","30.8","5.02","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（陂面镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-18","61","5","40","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（陂面镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-18","2.44","0.26","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（永宁镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水排放口(DW001)","总磷（以P计）","2022-01-18","4.31","0.14","0.5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（永宁镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","pH值","2022-01-18","7.0","7.0","9","6","无量纲","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（永宁镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","污水排放口(DW001)","氨氮（NH3-N）","2022-01-18","16.7","1.86","5","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（永宁镇生活污水处理站）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水排放口(DW001)","总氮（以N计）","2022-01-18","26.5","6.13","15","","mg/L","否","","","是"]
["2022年执法监测","阳春市碧源春环保科技有限公司（永宁镇生活污水处理站）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","污水排放口(DW001)","化学需氧量","2022-01-18","215","6","40","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","阴离子表面活性剂","2022-06-10","","<0.05","3","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","五日生化需氧量","2022-06-10","","4.8","15","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","化学需氧量","2022-06-10","","14","80","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","氨氮（NH3-N）","2022-06-10","","4.96","12","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","动植物油","2022-06-10","","<0.06","5","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区东钦羽毛加工厂","水环境","羽毛(绒)加工","","","综合废水排放口001(DW001)","悬浮物","2022-06-10","","8","30","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","化学需氧量","2022-06-10","","35","90","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","石油类","2022-06-10","","<0.06","5.0","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水总排放口(DW001)","动植物油","2022-06-10","","<0.06","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","悬浮物","2022-06-10","","9","60","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","五日生化需氧量","2022-06-10","","13.1","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,其他排污单位","废水总排放口(DW001)","氨氮（NH3-N）","2022-06-10","","1.20","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江珠江啤酒分装有限公司","水环境","制造业","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","废水总排放口(DW001)","pH值","2022-06-10","","7.9","9","6","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","总余氯","2022-06-10","","0.26","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","挥发酚","2022-06-10","","<0.01","1.0","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","色度","2022-06-10","","<2","","","倍","否","","","否"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","化学需氧量","2022-06-10","","52","250","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","粪大肠菌群","2022-06-10","","<20","5000","","个/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","pH值","2022-06-10","","7.9","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","悬浮物","2022-06-10","","10","60","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","五日生化需氧量","2022-06-10","","17.9","100","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","石油类","2022-06-10","","0.06","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","氰化物（总氰化合物）","2022-06-10","","<0.004","0.5","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","动植物油","2022-06-10","","0.15","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","阴离子表面活性剂（LAS）","2022-06-10","","<0.05","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","医疗机构水污染物排放标准(GB18466-2005)","（表2）综合医疗机构和其他医疗机构水污染物排放限值（日均值）,采用其他消毒方式,预处理标准","废水总排放口（DW001）","氨氮（NH3-N）","2022-06-10","","8.13","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","废水总排口","化学需氧量","2022-06-09","","7","40","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","总氮（以N计）","2022-06-09","","1.84","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","阴离子表面活性剂","2022-06-09","","<0.05","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","总铅","2022-06-09","","<0.001","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","总汞","2022-06-09","","0.00013","0.001","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","色度","2022-06-09","","<2","30","","倍","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","B标准","废水总排口","氨氮（NH3-N）","2022-06-09","","0.119","8","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","废水总排口","总磷（以P计）","2022-06-09","","0.38","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","烷基汞","2022-06-09","","<0.00003","0","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","动植物油","2022-06-09","","<0.06","3","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","五日生化需氧量","2022-06-09","","2.4","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","悬浮物","2022-06-09","","5","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","总铬","2022-06-09","","<0.03","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","六价铬","2022-06-09","","<0.004","0.05","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","pH值","2022-06-09","","7.8","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","总镉","2022-06-09","","<0.0001","0.01","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排口","石油类","2022-06-09","","<0.06","3","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区鑫泰源污水处理有限公司","","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排口","总砷","2022-06-09","","0.0007","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市保源环保有限公司","水环境","固体废物治理","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","氨氮","2022-06-10","","0.975","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市保源环保有限公司","水环境","固体废物治理","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","化学需氧量","2022-06-10","","162","500","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市保源环保有限公司","水环境","固体废物治理","","","废水排放口DW001","五日生化需氧量","2022-06-10","","47.4","300","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市保源环保有限公司","水环境","固体废物治理","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","悬浮物","2022-06-10","","4","400","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市惠和硅制品有限公司","水环境","专项化学用品制造","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","五日生化需氧量","2022-06-10","","7.8","300","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市惠和硅制品有限公司","水环境","专项化学用品制造","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","化学需氧量","2022-06-10","","21","500","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市惠和硅制品有限公司","水环境","专项化学用品制造","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","氨氮","2022-06-10","","0.616","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市惠和硅制品有限公司","水环境","专项化学用品制造","水污染物排放限值(DB44/26-2001)","第二时段三级标准","废水排放口DW001","悬浮物","2022-06-10","","4","400","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","pH值","2022-06-09","","7.2","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","色度","2022-06-09","","<2","30","","倍","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","化学需氧量","2022-06-09","","7","50","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","五日生化需氧量","2022-06-09","","2.3","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","悬浮物","2022-06-09","","4","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","总氮（以N计）","2022-06-09","","1.41","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","阴离子表面活性剂","2022-06-09","","<0.05","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铅","2022-06-09","","<0.001","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总汞","2022-06-09","","0.00012","0.001","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,2006年1月1日后建设","排放口(1)","总磷（以P计）","2022-06-09","","0.36","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","烷基汞","2022-06-09","","<0.00003","0","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","动植物油","2022-06-09","","0.09","3","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口(1)","石油类","2022-06-09","","<0.06","3","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总砷","2022-06-09","","0.0007","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总铬","2022-06-09","","<0.03","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","总镉","2022-06-09","","<0.0001","0.01","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口(1)","氨氮（NH3-N）","2022-06-09","","0.027","5;8","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森禾净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","排放口(1)","六价铬","2022-06-09","","<0.004","0.05","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口(DW001)","悬浮物","2022-06-20","","14","400","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口(DW001)","氨氮（NH3-N）","2022-06-20","","2.31","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口(DW001)","化学需氧量","2022-06-20","","56","500","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口(DW001)","五日生化需氧量","2022-06-20","","16.5","300","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东区森堡利制衣厂","水环境","其他机织服装制造","","","废水排放口DW001","总磷（以P计）","2022-06-10","","0.55","1.5","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区森堡利制衣厂","水环境","其他机织服装制造","","","废水排放口DW001","悬浮物","2022-06-10","","6","100","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区森堡利制衣厂","水环境","其他机织服装制造","","","废水排放口DW001","氨氮（NH3-N）","2022-06-10","","4.75","20","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区森堡利制衣厂","水环境","其他机织服装制造","","","废水排放口DW001","五日生化需氧量","2022-06-10","","8.2","50","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江市阳东区森堡利制衣厂","水环境","其他机织服装制造","","","废水排放口DW001","化学需氧量","2022-06-10","","23","200","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水排污口DW001(DW001)","pH值","2022-06-09","","7.4","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排污口DW001(DW001)","悬浮物","2022-06-09","","12","400","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排污口DW001(DW001)","化学需氧量","2022-06-09","","21","500","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排污口DW001(DW001)","石油类","2022-06-09","","<0.06","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排污口DW001(DW001)","五日生化需氧量","2022-06-09","","7.4","300","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江喜之郎果冻制造有限公司","水环境","其他未列明食品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排污口DW001(DW001)","氨氮（NH3-N）","2022-06-09","","3.73","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水排放口DW001(DW001)","pH值","2022-06-09","","8.5","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口DW001(DW001)","氨氮（NH3-N）","2022-06-09","","0.856","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口DW001(DW001)","化学需氧量","2022-06-09","","32","500","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口DW001(DW001)","石油类","2022-06-09","","<0.06","20","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口DW001(DW001)","悬浮物","2022-06-09","","6","400","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水排放口DW001(DW001)","磷酸盐（以P计）","2022-06-09","","0.01","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","","","废水排放口DW001(DW001)","总氮（以N计）","2022-06-09","","1.84","","","mg/L","否","","","否"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水排放口DW001(DW001)","动植物油","2022-06-09","","<0.06","100","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江十八子精密特钢有限公司","水环境,大气环境","黑色金属冶炼和压延加工业 ","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","废水排放口DW001(DW001)","色度","2022-06-09","","<2","","","度","否","","","否"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总氮（以N计）","2022-06-09","","2.46","15","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总砷","2022-06-09","","0.0008","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","氨氮（NH3-N）","2022-06-09","","<0.025","5;8","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总镉","2022-06-09","","<0.0001","0.01","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","动植物油","2022-06-09","","<0.06","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","石油类","2022-06-09","","<0.06","1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","六价铬","2022-06-09","","<0.004","0.05","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","烷基汞","2022-06-09","","<0.00003","0","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铅","2022-06-09","","<0.001","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","五日生化需氧量","2022-06-09","","1.5","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","色度","2022-06-09","","<2","30","","倍","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","pH值","2022-06-09","","7.2","9","6","无量纲","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","总铬","2022-06-09","","<0.03","0.1","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","阴离子表面活性剂","2022-06-09","","<0.05","0.5","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水总排放口(DW001)","总磷（以P计）","2022-06-09","","0.31","0.5","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","悬浮物","2022-06-09","","4","10","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,城镇二级污水处理厂","废水总排放口(DW001)","化学需氧量","2022-06-09","","5","40","","mg/L","否","","","是"]
["2022年阳东区执法监测","阳江市阳东迅捷水质净化有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","废水总排放口(DW001)","总汞","2022-06-09","","0.00018","0.001","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","海洋石油阳江实业有限公司","水环境","油气仓储","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水排放口(DW001)","石油类","2022-09-16","","0.35","8.0","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","海洋石油阳江实业有限公司","水环境","油气仓储","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","废水排放口(DW001)","pH值","2022-09-16","","7.9","9","6","无量纲","否","","","是"]
["2022年阳江高新区执法监测","海洋石油阳江实业有限公司","水环境","油气仓储","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水排放口(DW001)","悬浮物","2022-09-16","","4","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","海洋石油阳江实业有限公司","水环境","油气仓储","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水排放口(DW001)","氨氮（NH3-N）","2022-09-16","","0.065","15","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","海洋石油阳江实业有限公司","水环境","油气仓储","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","废水排放口(DW001)","化学需氧量","2022-09-16","","4","110","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","废水处理后出口","悬浮物","2022-09-15","","24","230","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,合成氨工业","废水处理后出口","氨氮（NH3-N）","2022-09-15","","8.69","25","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,纺织染整工业","废水处理后出口","化学需氧量","2022-09-15","","144","260","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","废水处理后出口","pH值","2022-09-15","","7.3","9","6","无量纲","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,三级标准,2005年12月31日前建设","废水处理后出口","总磷（以P计）","2022-09-15","","0.57","4","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,纺织染整、养殖、屠宰、肉制品加工","废水处理后出口","五日生化需氧量","2022-09-15","","40.2","150","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","废水处理后出口","色度","2022-09-15","","3","64","","倍","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,一切排污单位","废水处理后出口","动植物油","2022-09-15","","1.63","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市皇玛服饰有限公司","","服饰制造","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水处理后出口","总氮（以N计）","2022-09-15","","9.26","35","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","化学需氧量","2022-09-15","","11","260","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","悬浮物","2022-09-15","","4","230","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","总磷（以P计）","2022-09-15","","0.27","4","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","pH","2022-09-15","","7.9","9","6.5","无量纲","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","总氮（以N计）","2022-09-15","","5.49","35","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","阴离子表面活性剂（LAS）","2022-09-15","","0.09","10","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","五日生化需氧量","2022-09-15","","3.2","150","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","动植物油","2022-09-15","","0.21","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江和鲜食品有限公司","水环境","调味品、发酵制品制造","污水排入城镇下水道水质标准(GB/T31962-2015)","污水排入城镇下水道水质控制项目限值,C级","污水总排放口(DW001)","氨氮（NH3-N）","2022-09-15","","0.187","25","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆企业","废水监测点1","五日生化需氧量","2022-09-15","","14.9","40","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","废水监测点1","氨氮（NH3-N）","2022-09-15","","1.27","16","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","废水监测点1","pH值","2022-09-15","","7","9","6","无量纲","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,造纸企业","废水监测点1","总磷（以P计）","2022-09-15","","0.16","1.6","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表3）水污染物特别排放限值,企业自产废纸浆量占企业制浆总用量的比重不大于80%,企业废水总排放口,制浆与造纸联合生产企业","废水监测点1","悬浮物","2022-09-15","","4","60","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业漂白非木浆产量占企业纸浆总用量的比重大于60%,企业废水总排放口,制浆与造纸联合生产企业","废水监测点1","总氮（以N计）","2022-09-15","","8.68","24","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","维达护理用品（广东）有限公司","水环境","机制纸及纸板制造","制浆造纸工业水污染物排放标准(GB3544-2008)","（表1、表2）现有和新建企业水污染物排放标准,企业自产废纸浆量占企业制浆总用量的比重大于80%,企业废水总排放口,制浆和造纸联合生产企业","废水监测点1","化学需氧量","2022-09-15","","53","160","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","总磷（以P计）","2022-09-14","","0.42","2.0","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,其他排污单位","废水处理后出口","五日生化需氧量","2022-09-14","","48.4","150","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,一切排污单位","废水处理后出口","动植物油","2022-09-14","","0.07","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","化学需氧量","2022-09-14","","175","200","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","氨氮（NH3-N）","2022-09-14","","3.46","15","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","石油类","2022-09-14","","0.37","10","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","总锌","2022-09-14","","0.05","2","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口","六价铬","2022-09-14","","0.004","0.25","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","总铜","2022-09-14","","0.05","0.5","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","悬浮物","2022-09-14","","32","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口","总镍","2022-09-14","","0.05","0.5","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表1   第一类污染物最高允许排放浓度,一切排污单位","废水处理后出口","总铬","2022-09-14","","0.03","0.75","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),一级标准,一切排污单位","废水处理后出口","pH值","2022-09-14","","7","8","7","无量纲","否","","","是"]
["2022年阳江高新区执法监测","阳江开宝新材料实业有限公司","水环境,土壤环境","金属表面处理及热处理加工","钢铁工业水污染物排放标准(GB13456-2012)","（表1、表2）现有和新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,间接排放限值","废水处理后出口","总氮（以N计）","2022-09-14","","7.39","35","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,天然橡胶乳加工、酒精、味精、皮革、化纤浆粕工业","生产废水排放口(DW002)","五日生化需氧量","2022-09-15","","53.6","150","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","生产废水排放口(DW002)","pH","2022-09-15","","8.1","9","6.5","无量纲","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准（勿选）(DB44/26-2001)","第二类污染物最高允许排放浓度","生产废水排放口(DW002)","总磷（以P计）","2022-09-15","","0.89","4","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","水污染物排放限值(DB44/26-2001)","第二时段三级标准","生产废水排放口(DW002)","氨氮","2022-09-15","","3.24","25","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,生物制药、皮革、苎麻脱胶、化纤浆粕、天然橡胶乳加工工业","生产废水排放口(DW002)","化学需氧量","2022-09-15","","198","260","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),三级标准,制浆、制浆造纸、造纸","生产废水排放口(DW002)","悬浮物","2022-09-15","","66","230","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表2   第二类污染物最高允许排放浓度 (第一时段),二级标准,一切排污单位","生产废水排放口(DW002)","动植物油","2022-09-15","","0.11","100","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,一切排污单位","生产废水排放口(DW002)","色度","2022-09-15","","8","64","","倍","否","","","是"]
["2022年阳江高新区执法监测","阳江市金彭服饰实业有限公司","水环境,大气环境","服饰制造","水污染物排放限值标准（勿选）(DB44/26—2001)","表2 第二类污染物最高允许排放浓度,第一时段,一级标准","生产废水排放口(DW002)","总氮（以N计）","2022-09-15","","4.30","35","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","总氮（以N计）","2022-08-30","","8.25","15","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","化学需氧量","2022-08-30","","8","40","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","石油类","2022-08-30","","0.15","1","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表2）部分一类污染物最高允许排放浓度（日均值）","J2021030125-1-1-001","总汞","2022-08-30","","0.00017","0.001","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","氨氮（NH3-N）","2022-08-30","","0.635","5","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","总铬","2022-08-30","","0.03","0.1","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","J2021030125-1-1-001","pH值","2022-08-30","","7.1","9","6","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","悬浮物","2022-08-30","","4","10","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,一切排污单位","J2021030125-1-1-001","色度","2022-08-30","","2","30","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","J2021030125-1-1-001","总磷（以P计）","2022-08-30","","0.07","0.5","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","五日生化需氧量","2022-08-30","","2.4","10","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","总砷","2022-08-30","","0.0003","0.1","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","粪大肠菌群数","2022-08-30","","0.049","1000","","个/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","总铅","2022-08-30","","0.01","0.1","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","总镉","2022-08-30","","0.001","0.01","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","六价铬","2022-08-30","","0.004","0.05","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,二级标准（水温＞12℃或≤12℃）,通用","J2021030125-1-1-001","阴离子表面活性剂（LAS）","2022-08-30","","0.09","0.5","","mg/L","否","","","是"]
["2022年阳江高新区执法监测","阳江市新环水务有限公司(阳江高新区第一污水处理厂）","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","J2021030125-1-1-001","动植物油","2022-08-30","","0.33","1","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,车间生产设施废水排放口","总排放口(DW004)","六价铬","2022-09-05","","<0.004","0.1","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","总磷（以P计）","2022-09-05","","0.16","1","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","化学需氧量","2022-09-05","","21","100","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","氨氮（NH3-N）","2022-09-05","","7.21","25","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,企业废水总排放口,直接排放限值,制革企业","总排放口(DW004)","pH值","2022-09-05","","6.6","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","阳西县长江制革有限公司","水环境","皮革鞣制加工","制革及毛皮加工工业水污染物排放标准(GB30486-2013)","（表2）新建企业水污染物排放浓度限值及单位产品基准排水量,车间生产设施废水排放口","总排放口(DW004)","总铬","2022-09-05","","<0.03","1.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","悬浮物","2022-12-19","","7","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","氨氮（NH3-N）","2022-12-19","","2.60","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水处理后排放口001(DW001)","总磷（以P计）","2022-12-19","","0.47","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","pH值","2022-12-19","","7.0","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","污水处理后排放口001(DW001)","化学需氧量","2022-12-19","","24","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县上洋镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","总氮（以N计）","2022-12-19","","9.84","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","pH值","2022-12-19","","6.8","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","悬浮物","2022-12-19","","9","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","总氮（以N计）","2022-12-19","","8.89","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","污水处理后排放口001(DW001)","化学需氧量","2022-12-19","","22","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","氨氮（NH3-N）","2022-12-19","","0.442","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县程村镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水处理后排放口001(DW001)","总磷（以P计）","2022-12-19","","0.28","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","A标准","总排放口(1)","氨氮（NH3-N）","2022-12-19","","1.64","5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","悬浮物","2022-12-19","","7","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","总排放口(1)","pH值","2022-12-19","","6.9","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","总排放口(1)","化学需氧量","2022-12-19","","23","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","总排放口(1)","总氮（以N计）","2022-12-19","","8.00","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西捷晖净水有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","总排放口(1)","总磷（以P计）","2022-12-19","","0.20","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","香山家园污水处理厂废水处理后出水口","悬浮物","2022-12-19","","9","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","香山家园污水处理厂废水处理后出水口","pH值","2022-12-19","","6.8","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","香山家园污水处理厂废水处理后出水口","总氮（以N计）","2022-12-19","","10.1","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","香山家园污水处理厂废水处理后出水口","氨氮（NH3-N）","2022-12-19","","0.240","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","香山家园污水处理厂废水处理后出水口","总磷（以P计）","2022-12-19","","0.49","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县香山家园污水处理有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","香山家园污水处理厂废水处理后出水口","化学需氧量","2022-12-19","","15","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","悬浮物","2022-12-19","","8","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","pH值","2022-12-19","","6.9","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","氨氮（NH3-N）","2022-12-19","","1.41","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","污水处理后排放口001(DW001)","化学需氧量","2022-12-19","","18","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","总氮（以N计）","2022-12-19","","7.76","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县塘口镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水处理后排放口001(DW001)","总磷（以P计）","2022-12-19","","0.31","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","污水处理设施出口","化学需氧量","2022-11-10","","80","500","","mg/L","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),二级标准,其他排污单位","污水处理设施出口","氨氮（NH3-N）","2022-11-10","","2.83","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","污水处理设施出口","五日生化需氧量","2022-11-10","","31.4","300","","mg/L","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,其他排污单位","污水处理设施出口","悬浮物","2022-11-10","","4","400","","mg/L","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","污水处理设施出口","pH值","2022-11-10","","7.1","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","广东厨邦食品有限公司","水环境","酱油、食醋及类似制品制造","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),三级标准,一切排污单位","污水处理设施出口","动植物油","2022-11-10","","0.07","100","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","总氮（以N计）","2022-12-19","","8.02","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","氨氮（NH3-N）","2022-12-19","","1.07","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","污水处理后排放口001(DW001)","总磷（以P计）","2022-12-19","","0.20","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","pH值","2022-12-19","","6.9","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","污水处理后排放口001(DW001)","化学需氧量","2022-12-19","","28","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","建广环境葛洲坝水务（阳西）有限公司-阳西县新墟镇污水处理厂","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","污水处理后排放口001(DW001)","悬浮物","2022-12-19","","7","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","水环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","化学需氧量","2022-09-05","","<4","100","","mg/L","否","","","是"]
["2022年阳西分局执法监测","东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","水环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","总磷（以P计）","2022-09-05","","0.05","3","","mg/L","否","","","是"]
["2022年阳西分局执法监测","东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","水环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","总铬","2022-09-05","","<0.03","0.1","","mg/L","否","","","是"]
["2022年阳西分局执法监测","东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","水环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物特别排放限值","总排放口(DW001)","六价铬","2022-09-05","","<0.004","0.05","","mg/L","否","","","是"]
["2022年阳西分局执法监测","东莞市园林绿化工程有限公司（阳西县生活垃圾卫生填埋场）","水环境","环境卫生管理","生活垃圾填埋场污染控制标准(GB16889-2008)","现有和新建生活垃圾填埋场水污染物排放浓度限值","总排放口(DW001)","氨氮（NH3-N）","2022-09-05","","0.246","25","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","废水总排放口(DW001)","化学需氧量","2022-12-19","","20","40","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","氨氮（NH3-N）","2022-12-19","","0.692","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","废水总排放口(DW001)","总氮（以N计）","2022-12-19","","13.0","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","废水总排放口(DW001)","总磷（以P计）","2022-12-19","","0.42","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","悬浮物","2022-12-19","","7","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西县百奥污水处理有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","废水总排放口(DW001)","pH值","2022-12-19","","6.9","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","总氮（以N计）","2022-12-19","","10.8","15","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","氨氮（NH3-N）","2022-12-19","","0.418","5;8","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,2006年1月1日后建设","排放口","总磷（以P计）","2022-12-19","","0.44","0.5","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,A标准,通用","排放口","悬浮物","2022-12-19","","8","10","","mg/L","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","城镇污水处理厂污染物排放标准[国标](GB18918-2002)","（表1）基本控制项目最高允许排放浓度（日均值）,一级标准（水温＞12℃或≤12℃）,B标准,通用","排放口","pH值","2022-12-19","","6.9","9","6","无量纲","否","","","是"]
["2022年阳西分局执法监测","阳西中炬水务有限公司","水环境","污水处理及其再生利用","广东省水污染排放限值标准(DB44/26—2001)","表4   第二类污染物最高允许排放浓度 (第二时段),一级标准,城镇二级污水处理厂","排放口","化学需氧量","2022-12-19","","26","40","","mg/L","否","","","是"]

{"sheet":"无组织","index":2,"n_rows":34,"n_cols":20,"rows_kept":34,"merged":[[1,0,33,0],[1,1,4,1],[5,1,16,1],[17,1,21,1],[22,1,25,1],[26,1,29,1],[30,1,33,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","风向","风速（m/s）","温度(℃)","压力（kPa）","排放浓度","上限","下限","单位","是否超标","超标倍数","备注"]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","下风向监测点3#","臭气浓度","2022-07-01","东风","1.0","31.2","101.9","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","下风向监测点4#","臭气浓度","2022-07-01","东风","1.0","31.2","101.9","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","上风向监测点1#","臭气浓度","2022-07-01","东风","1.0","31.2","101.9","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市伟艺抛磨材料有限公司","大气环境","制造业","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","下风向监测点2#","臭气浓度","2022-07-01","东风","1.0","31.2","101.9","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点2#","氨","2022-06-23","南","1.5","30.5","101","0.048","1.5","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点2#","硫化氢","2022-06-23","南","1.5","30.5","101","<0.0002","0.06","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点2#","臭气浓度","2022-06-23","南","1.5","30.5","101","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点3#","臭气浓度","2022-06-23","南","1.5","30.5","101","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点3#","氨","2022-06-23","南","1.5","30.5","101","0.053","1.5","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点3#","硫化氢","2022-06-23","南","1.5","30.5","101","<0.0002","0.06","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点4#","臭气浓度","2022-06-23","南","1.5","30.5","101","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点4#","硫化氢","2022-06-23","南","1.5","30.5","101","<0.0002","0.06","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点4#","氨","2022-06-23","南","1.5","30.5","101","0.050","1.5","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织上风向参照点1#","氨","2022-06-23","南","1.5","30.5","101","0.041","1.5","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织上风向参照点1#","硫化氢","2022-06-23","南","1.5","30.5","101","<0.0002","0.06","","mg/m3","否","",""]
["2022年阳东区执法监测","阳东区人民医院","水环境","综合医院","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织上风向参照点1#","臭气浓度","2022-06-23","南","1.5","30.5","101","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点4#","臭气浓度","2022-06-20","西南","2.3","29.2","100.6","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点3#","臭气浓度","2022-06-20","西南","2.3","29.2","100.6","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","","","厂界无组织上风向参照点1#","臭气浓度","2022-06-20","西南","2.3","29.2","100.6","<10","","","mg/Nm3","否","",""]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织上风向参照点1#","臭气浓度","2022-06-20","西南","2.3","29.2","100.6","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市金江环境有限公司","水环境,大气环境","危险废物治理","恶臭污染物排放标准(GB14554-93)","（表1）恶臭污染物厂界标准值,二级,新扩改建","厂界无组织下风向监测点2#","臭气浓度","2022-06-20","西南","2.3","29.2","100.6","<10","20","","无量纲","否","",""]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织上风向监测点1#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","东南","1.9","32.7","100.8","0.092","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点2#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","东南","1.9","32.7","100.8","0.129","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点3#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","东南","1.9","32.7","100.8","0.103","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区恒丰环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点4#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","东南","1.9","32.7","100.8","0.113","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","上风向1#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-23","南","1.6","31.2","100.8","0.090","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","下风向4#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-23","南","1.6","31.2","100.8","0.110","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","下风向2#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-23","南","1.6","31.2","100.8","0.129","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东新洲新高腾环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","下风向3#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-23","南","1.6","31.2","100.8","0.114","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点2#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","南","1.7","31.1","100.9","0.084","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点3#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","南","1.7","31.1","100.9","0.110","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织上风向参照点1#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","南","1.7","31.1","100.9","0.119","1.0","","mg/m3","否","",""]
["2022年阳东区执法监测","阳江市阳东区源福新型环保建材有限公司","大气环境","粘土砖瓦及建筑砌块制造","砖瓦工业大气污染物排放标准(GB29620-2013)","（表3）现有和新建企业边界大气污染浓度限值","厂界无组织下风向监测点4#","总悬浮颗粒物（空气动力学当量直径100μm以下）","2022-06-22","南","1.7","31.1","100.9","0.103","1.0","","mg/m3","否","",""]

{"sheet":"周边环境","index":3,"n_rows":37,"n_cols":21,"rows_kept":37,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,12],[0,13,1,13],[0,14,1,14],[0,15,1,15],[0,16,1,16],[0,17,1,17],[0,18,1,18],[0,19,1,19],[0,20,1,20],[2,0,36,0],[2,1,18,1],[19,1,36,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","周边环境-土壤","周边环境-土壤","周边环境-土壤","周边环境-土壤","折算/浓度/昼间","夜间","上限","下限","单位","是否超标","超标倍数","备注"]
["","","","","","","","","","土壤颜色","土壤水分(%)","利用情况","土壤pH值","","","","","","","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","铬（六价）","2022-06-15","红棕色","","","","<0.5","","78","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","苯并(a)蒽","2022-06-15","红棕色","","","","<0.1","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","β-六六六","2022-06-15","红棕色","","","","<0.05","","9.2","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","铜","2022-06-15","红棕色","","","","6","","36000","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","苯并(k)荧蒽","2022-06-15","红棕色","","","","<0.1","","1500","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","苯并(b)荧蒽","2022-06-15","红棕色","","","","<0.2","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","铅","2022-06-15","红棕色","","","","29.8","","2500","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","二苯并(a,h)蒽","2022-06-15","红棕色","","","","<0.1","","15","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","镍 ","2022-06-15","红棕色","","","","9","","2000","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","砷","2022-06-15","红棕色","","","","0.84","","140","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","苯并(a)芘","2022-06-15","红棕色","","","","<0.1","","15","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","滴滴涕","2022-06-15","红棕色","","","","<0.26","","67","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","汞","2022-06-15","红棕色","","","","0.033","","82","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","镉","2022-06-15","红棕色","","","","0.04","","172","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","α-六六六","2022-06-15","红棕色","","","","<0.06","","3","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","γ-六六六","2022-06-15","红棕色","","","","<0.06","","19","","mg/KG","否","",""]
["2022年阳东区执法监测","广东省粤钢新材料科技有限公司","土壤环境","其他金属制日用品制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","广东省粤钢新材料科技有限公司","茚并[1，2，3-cd]芘","2022-06-15","红棕色","","","","<0.1","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","苯并(a)芘","2022-06-13","暗灰色","","","","<0.1","","15","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","镉","2022-06-13","暗灰色","","","","0.14","","172","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","α-六六六","2022-06-13","暗灰色","","","","<0.06","","3","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","β-六六六","2022-06-13","暗灰色","","","","<0.05","","9.2","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","铜","2022-06-13","暗灰色","","","","11","","36000","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","苯并(k)荧蒽","2022-06-13","暗灰色","","","","<0.1","","1500","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","","","阳江市金恒实业有限公司","阳离子交换量","2022-06-13","暗灰色","","","","3.3","","","","mg/L","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","镍 ","2022-06-13","暗灰色","","","","13","","2000","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","汞","2022-06-13","暗灰色","","","","0.012","","82","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","滴滴涕","2022-06-13","暗灰色","","","","<0.26","","67","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","砷","2022-06-13","暗灰色","","","","2.38","","140","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","铅","2022-06-13","暗灰色","","","","29.1","","2500","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","苯并(b)荧蒽","2022-06-13","暗灰色","","","","<0.2","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","二苯并(a,h)蒽","2022-06-13","暗灰色","","","","<0.1","","15","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","苯并(a)蒽","2022-06-13","暗灰色","","","","<0.1","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","茚并[1，2，3-cd]芘","2022-06-13","暗灰色","","","","<0.1","","151","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表1 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","铬（六价）","2022-06-13","暗灰色","","","","<0.5","","78","","mg/KG","否","",""]
["2022年阳东区执法监测","阳江市金恒实业有限公司","土壤环境","金属结构制造","土壤环境质量建设用地土壤污染风险管控标准标准(试行)(GB36600-2018)","表2 建设用地土壤污染风险筛选值与管制值（基本项目）,第二类用地-管制值","阳江市金恒实业有限公司","γ-六六六","2022-06-13","暗灰色","","","","<0.06","","19","","mg/KG","否","",""]

{"sheet":"厂界噪声","index":4,"n_rows":4,"n_cols":19,"rows_kept":4,"merged":[[1,0,3,0],[1,1,2,1]],"flags":["formulas_cached_only"]}
["任务名称","企业名称","名录类别","行业类别","执行标准名称","执行标准条目名称","监测点","监测项目","监测日期","声源","风速（m/s）","昼间监测值","夜间监测值","上限","下限","单位","是否超标","超标倍数","备注"]
["2022年执法监测","阳春市豪达纸业有限公司","水环境","机制纸及纸板制造","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂界北面","工业企业厂界环境噪声","2022-07-12","机械声","1.7","59.3","60","60;50","","dB","是",";0.20",""]
["2022年执法监测","阳春市豪达纸业有限公司","水环境","机制纸及纸板制造","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂界西面","工业企业厂界环境噪声","2022-07-12","机械声","1.7","64","65","60;50","","dB","是","0.07;0.30",""]
["2022年执法监测","阳江市众鑫环保实业有限公司","大气环境,声环境","其他建筑材料制造","工业企业厂界环境噪声排放标准(GB12348-2008)","（表1）工业企业厂界环境噪声排放限值,厂界与噪声敏感建筑物距离不小于1m,2类厂界外声环境功能区,昼间/夜间","厂界南面","工业企业厂界环境噪声","2022-04-07","交通","1.7","59.4","51","60;50","","dB","是",";0.02","夜间噪声测量值为51dB，背景值为50.8，根据噪声测量值修正技术规范，51-50＜4，判定为达标。"]